# Invalid SPEC® CFP2006 Result

Copyright 2006-2023 Standard Performance Evaluation Corporation

Hygon

SPECfp®2006 = Not Run

SPECfp_base2006 = 40.7

CPU2006 license: | 0 | Test date: | Nov-2023
Test sponsor: |  | Hardware Availability: | May-2018
Tested by: |  | Software Availability: | Nov-2017

Hardware
CPU Name: | Hygon
CPU Characteristics: | Turbo CORE technology up to 3.00 GHz
CPU MHz: | 2000
FPU: | Integrated
CPU(s) enabled: | 64 cores, 2 chips, 32 cores/chip, 2 threads/core
CPU(s) orderable: | 1,2 chips
Primary Cache: | 64 KB I + 32 KB D on chip per core
Secondary Cache: | 512 KB I+D on chip per core
L3 Cache: | 64 MB I+D on chip per chip, 8 MB shared / 4 cores
Other Cache: | None
Memory: | 512 GB (16 x 64 GB 4Rx4 PC4-2933V-R), running at 2400)
Disk Subsystem: | 1 x 1000 GB SATA
Other Hardware: | None

Software
Operating System: | ubuntu 16.04 Kernel 4.4.0-116-generic
Compiler: | C/C++/Fortran: Version 4.5.2.1-1 of x86 Open64 Compiler Suite (from AMD)
Auto Parallel: | No
File System: | ext4
System State: | Run level 3 (Full multiuser with network)
Base Pointers: | 64-bit
Peak Pointers: | 32/64-bit
Other Software: | None

## Errors

    'reportable' flag not set during run
    465.tonto (base) did not have enough runs!
    453.povray (base) did not have enough runs!
    444.namd (base) did not have enough runs!
    416.gamess (base) did not have enough runs!
    436.cactusADM (base) did not have enough runs!
    459.GemsFDTD (base) did not have enough runs!
    450.soplex (base) did not have enough runs!
    437.leslie3d (base) did not have enough runs!
    447.dealII (base) did not have enough runs!
    481.wrf (base) did not have enough runs!
    433.milc (base) did not have enough runs!
    410.bwaves (base) did not have enough runs!
    435.gromacs (base) did not have enough runs!
    482.sphinx3 (base) did not have enough runs!
    434.zeusmp (base) did not have enough runs!
    470.lbm (base) did not have enough runs!
    454.calculix (base) did not have enough runs!

## Results Table

Benchmark | Base | Peak
--- | --- | ---
Seconds | Ratio | Seconds | Ratio | Seconds | Ratio | Seconds | Ratio | Seconds | Ratio | Seconds | Ratio
Results appear in the order in which they were run. Bold underlined text indicates a median measurement.
410.bwaves | 212 | 64.2 |  |  |  |  |  |  |  |  |  |
416.gamess | 711 | 27.6 |  |  |  |  |  |  |  |  |  |
433.milc | 174 | 52.6 |  |  |  |  |  |  |  |  |  |
434.zeusmp | 213 | 42.8 |  |  |  |  |  |  |  |  |  |
435.gromacs | 275 | 25.9 |  |  |  |  |  |  |  |  |  |
436.cactusADM | 184 | 64.9 |  |  |  |  |  |  |  |  |  |
437.leslie3d | 191 | 49.3 |  |  |  |  |  |  |  |  |  |
444.namd | 400 | 20.0 |  |  |  |  |  |  |  |  |  |
447.dealII | 226 | 50.6 |  |  |  |  |  |  |  |  |  |
450.soplex | 266 | 31.4 |  |  |  |  |  |  |  |  |  |
453.povray | 177 | 30.1 |  |  |  |  |  |  |  |  |  |
454.calculix | 219 | 37.7 |  |  |  |  |  |  |  |  |  |
459.GemsFDTD | 238 | 44.6 |  |  |  |  |  |  |  |  |  |
465.tonto | 302 | 32.6 |  |  |  |  |  |  |  |  |  |
470.lbm | 258 | 53.4 |  |  |  |  |  |  |  |  |  |
481.wrf | 205 | 54.4 |  |  |  |  |  |  |  |  |  |
482.sphinx3 | 426 | 45.7 |  |  |  |  |  |  |  |  |  |

## Submit Notes

    'numactl' was used to bind copies to the cores.
    See the configuration file for details.

## Operating System Notes

    'ulimit -s unlimited' was used to set environment stack size
    'ulimit -l 2097152' was used to set environment locked pages in memory limit

    runspec command invoked through numactl i.e.:
    numactl --interleave=all runspec <etc>

    Set dirty_ratio=8 to limit dirty cache to 8% of memory
    Set swappiness=1 to swap only if necessary
    Set zone_reclaim_mode=1 to free local node memory and avoid remote memory
    sync then drop_caches=3 to reset caches before invoking runcpu

    Transparent huge pages were enabled for this run (OS default)

    Set vm/nr_hugepages=114688 in /etc/sysctl.conf
    mount -t hugetlbfs nodev /mnt/hugepages

## Platform Notes

    BIOS settings:
    Determinism Slider = Power
    cTDP Control = Manual
    cTDP = 200
    This system Sugon A620-G30 is electrically equivalent to Sugon A420-G30 populated with the same processors and memories. This result is tested on a Sugon A620-G30 system.

## General Notes

    Environment variables set by runspec before the start of the run:
    HUGETLB_LIMIT = "896"
    LD_LIBRARY_PATH = "/home/speccpu2006/rate-libs-revB/32:/home/speccpu2006/rate-libs-revB/64"

    The binaries were built with the AMD supported x86 Open64 Compiler Suite,
    which is only available from AMD at
    http://developer.amd.com/tools-and-sdks/cpu-development/x86-open64-compiler-suite/
    Binaries were compiled on a system with 2 x Hygon chips + 256 GB Memory using CENTOS 6.5

## Base Compiler Invocation

### C benchmarks:

| opencc

### C++ benchmarks:

| openCC

### Fortran benchmarks:

| openf95

### Benchmarks using both Fortran and C:

| opencc openf95

## Base Portability Flags

410.bwaves: | -DSPEC_CPU_LP64
416.gamess: | -DSPEC_CPU_LP64
433.milc: | -DSPEC_CPU_LP64
434.zeusmp: | -DSPEC_CPU_LP64
435.gromacs: | -DSPEC_CPU_LP64
436.cactusADM: | -DSPEC_CPU_LP64 -fno-second-underscore
437.leslie3d: | -DSPEC_CPU_LP64
444.namd: | -DSPEC_CPU_LP64
447.dealII: | -DSPEC_CPU_LP64
450.soplex: | -DSPEC_CPU_LP64
453.povray: | -DSPEC_CPU_LP64
454.calculix: | -DSPEC_CPU_LP64
459.GemsFDTD: | -DSPEC_CPU_LP64
465.tonto: | -DSPEC_CPU_LP64
470.lbm: | -DSPEC_CPU_LP64
481.wrf: | -DSPEC_CPU_LINUX -DSPEC_CPU_CASE_FLAG -DSPEC_CPU_LP64 -fno-second-underscore
482.sphinx3: | -DSPEC_CPU_LP64

## Base Optimization Flags

### C benchmarks:

| -Ofast -OPT:malloc_alg=1 -HP:bd=2m:heap=2m -IPA:plimit=8000 -IPA:small_pu=100 -mso -march=bdver1 -mno-fma4 -mno-xop -mno-tbm -WB, -Wl, -z,muldefs -L/root/jemalloc/lib64/lib -ljemalloc

### C++ benchmarks:

| -Ofast -static -CG:load_exe=0 -OPT:malloc_alg=1 -INLINE:aggressive=on -HP:bd=2m:heap=2m -D__OPEN64_FAST_SET -march=bdver2 -mno-fma4 -mno-xop -mno-tbm -WB, -Wl, -z,muldefs -L/root/jemalloc/lib64/lib -ljemalloc -pthread -ldl -l rt

### Fortran benchmarks:

| -Ofast -LNO:blocking=off -LNO:simd_peel_align=on -OPT:rsqrt=2 -OPT:unroll_size=256 -HP:bd=2m:heap=2m -mso -march=bdver1 -mno-fma4 -mno-xop -mno-tbm -WB, -Wl, -z,muldefs -L/root/jemalloc/lib64/lib -ljemalloc

### Benchmarks using both Fortran and C:

| -Ofast -OPT:malloc_alg=1 -HP:bd=2m:heap=2m -IPA:plimit=8000 -IPA:small_pu=100 -mso -march=bdver1 -mno-fma4 -mno-xop -mno-tbm -WB, -Wl, -z,muldefs -LNO:blocking=off -LNO:simd_peel_align=on -OPT:rsqrt=2 -OPT:unroll_size=256 -L/root/jemalloc/lib64/lib -ljemalloc

W3C XHTML 1.0
W3C CSS